|  |  |  |
| --- | --- | --- |
| **FIGURE NO.** | **FIGURE NAME/CAPTION** | **PAGE NO.** |
| **Fig 1.1** | **Ordinary Wheelchair** | **12** |
| **Fig 1.2** | **Disabled People** | **13** |
| **Fig 2.1** | **Group of Disabled Children** | **14** |
| **Fig 2.2** | **Pie Chart of Causes of Disability** | **15** |
| **Fig 2.3** | **Health Sector Icon** | **16** |
| **Fig 2.4** | **Statistical overview of Disabilities** | **17** |
| **Fig 3.1** | **Frido GO Self Propelled Wheelchair** | **18** |
| **Fig 3.2** | **Kosmo Care Rider Wheelchair** | **19** |
| **Fig 3.3** | **Kosmo Care Recliner Junior** | **20** |
| **Fig 3.4** | **Freedom Power Wheelchair A08L** | **21** |
| **Fig 3.5** | **Wheelchair Model** | **22** |
| **Fig 4.1** | **Transmitter Block Diagram** | **23** |
| **Fig 4.2** | **Receiver Block Diagram** | **23** |
| **Fig 5.1** | **Transmitter Circuit Diagram** | **25** |
| **Fig 5.2** | **Receiver Circuit Diagram** | **25** |
| **Fig 6.1.1** | **Arduino Nano** | **27** |
| **Fig 6.1.2** | **Pin Diagram of Arduino Nano** | **28** |
| **Fig 6.2.1** | **MPU6050 3 Axis Gyro Sensor and Accelerometer** | **30** |
| **Fig 6.2.2** | **MPU6050 Pin Diagram** | **31** |
| **Fig 6.3.1** | **HC-05 Bluetooth Module** | **33** |
| **Fig 6.3.2** | **HC-05 Pin Diagram** | **33** |
| **Fig 6.3.3** | **Interfacing Bluetooth** | **34** |
| **Fig 6.4.1** | **Arduino Uno** | **35** |
| **Fig 6.4.2** | **Arduino Uno Pin Diagram** | **35** |
| **Fig 6.5.1** | **L298N Motor Driver** | **37** |
| **Fig 6.5.2** | **L298N Pin Diagram** | **38** |
| **Fig 6.6** | **Single Shaft BO Motor** | **39** |
| **Fig 6.7.1** | **Arduino IDE** | **40** |
| **Fig 6.7.2** | **Blink Example** | **40** |

|  |  |  |
| --- | --- | --- |
| **TABLE NO.** | **TABLE NAME/CAPTION** | **PAGE NO.** |
| **Table 6.1** | Arduino Nano Features | **29** |
| **Table 6.3** | **HC-05 Command Modes** | **34** |
| **Table 6.4** | **Arduino Uno Features** | **36** |
| **Table 6.5** | **L298N Pin Descriptions** | **38** |

|  |  |
| --- | --- |
| I2C | INTER INTEGRATED CIRCUIT |
| CRPD | Convention on the Rights of Persons with Disabilities |
| COVID-19 | coronavirus disease |
| WHO | World Health Organization |
| UN | UNITE NATIONS |
| UNICEF | United Nations Children's Fund |
| Kg | KILOGRAMS |
| Lbs | Pound |
| ₹ | Rupees |
| Li-Po | lithium-polymer |
| RPM | Revolutions per minute |
| IDE | integrated development environment |
| KB | KILOBYTES |
| EEPROM | ELECTRONICALLY ERASABLE PROGRAMMABLE READ ONLY MEMORY |
| SRAM | STATIC RANDOM-ACCESS MEMORY |
| PWM | PULSE WIDTH MODULATION |
| USB | UNIVERSAL SERIAL BUS |
| UART | UNIVERSAL ASYNCHRONOUS RECEIVER TRANSMITTER |
| SS | SLAVE SELECT |
| SCK/SCL | SERIAL CLOCK |
| SDA | SERIAL DATA |
| MHz | MEGAHERTZ |
| MISO | MASTER INPUT SLAVE OUTPUT |
| MOSI | MASTER OUTPUT SLAVE INPUT |
| LED | LIGHT EMITTING DIODE |
| PCB | PRINTED CIRCUIT BOARD |
| I.E | THAT IS |
| A | AMPERE |
| C | CURRENT |
| CM | CENTIMETER |
| DC | DIRECT CURRENT |
| Vin | VOLTAGE INPUT |
| GND | GROUND |
| MA | MILLIAMPERE |